Highlights

**Optimal monitoring design for uncertainty quantification during geologic CO2 sequestration: A machine learning approach**

Misael M. Morales, Mohamed Mehana, Carlos Torres-Verdin, Michael J. Pyrcz, and Bailian Chen

* Filtering-based data assimilation method is developed to perform monitoring design.
* Machine learning reduced-order model is used to reduce computational cost of data assimilation process.
* Optimal monitoring design is obtained by optimizing the monitoring well location and monitoring measurement type to reduce the uncertainty in leakage risks prediction.